; Copyright (C), Intel Corporation. All rights reserved. 
; ********************************************************************************************** 
; **    Filename:  iaAHCIC.inf 
; **    Revision:  07/23/2021,18.36.1.1016
; **    Abstract:  Windows* INF File for AHCI Intel(R) Rapid Storage Technology Driver 
; **               Installs: RST AHCI Controller Miniport
; ********************************************************************************************** 
[Version] 
Signature="$Windows NT$" 
Provider=%INTEL% 
ClassGUID={4D36E96A-E325-11CE-BFC1-08002BE10318}
Class=HDC
CatalogFile=iaAHCIC.cat
DriverVer=07/23/2021,18.36.1.1016
PnpLockDown=1

;*************************************
;* Source files and copy sections
;*************************************
[SourceDisksNames]
1 = %DiskId1%,,,""

[SourceDisksFiles.amd64]
iaStorAC.sys = 1,,,
RstMwService.exe = 1,,,
RstMwEventLogMsg.dll = 1,,,

[DestinationDirs]
DefaultDestDir = 13
Driver_files_copy = 12
RstMwService_EventLog_files_copy = 11

[Driver_files_copy]
iaStorAC.sys

[RstMwService_EventLog_files_copy]
RstMwEventLogMsg.dll

;*************************************
;* Manufacturer and Model sections
;*************************************
[Manufacturer]
%INTEL% = INTEL, NTamd64.10.0...15063

[INTEL.NTamd64.10.0...15063]
%PCI\VEN_8086&DEV_A282&CC_0106.DeviceDesc% = AHCI_inst, PCI\VEN_8086&DEV_A282&CC_0106
%PCI\VEN_8086&DEV_34D3&CC_0106.DeviceDesc% = AHCI_inst, PCI\VEN_8086&DEV_34D3&CC_0106
%PCI\VEN_8086&DEV_02D3&CC_0106.DeviceDesc% = AHCI_inst, PCI\VEN_8086&DEV_02D3&CC_0106
%PCI\VEN_8086&DEV_06D2&CC_0106.DeviceDesc% = AHCI_inst, PCI\VEN_8086&DEV_06D2&CC_0106
%PCI\VEN_8086&DEV_06D3&CC_0106.DeviceDesc% = AHCI_inst, PCI\VEN_8086&DEV_06D3&CC_0106
%PCI\VEN_8086&DEV_A382&CC_0106.DeviceDesc% = AHCI_inst, PCI\VEN_8086&DEV_A382&CC_0106
%PCI\VEN_8086&DEV_43D2&CC_0106.DeviceDesc% = AHCI_inst, PCI\VEN_8086&DEV_43D2&CC_0106

;******************************************************************************
;*
;* RST AHCI Controller install section
;*
;******************************************************************************
[AHCI_inst.NTamd64]
CopyFiles=Driver_files_copy
CopyFiles=@RstMwService.exe
CopyFiles=RstMwService_EventLog_files_copy
FeatureScore=0x80

[AHCI_inst.ntamd64.Services]
AddService = iaStorAC, %SPSVCINST_ASSOCSERVICE%, iaStorAC_inst, iaStorAC_EventLog_inst
AddService = RstMwService, 0x00000000, RstMwService_inst, RstMwService_EventLog_inst, System, %RstMwService.EventLogSourceName%

;*************************************
;* Service: iaStorAC
;*************************************
[iaStorAC_inst] 
DisplayName    = %iaStorAC.ServiceName%
ServiceType    = %SERVICE_KERNEL_DRIVER% 
StartType      = %SERVICE_BOOT_START% 
ErrorControl   = %SERVICE_ERROR_NORMAL% 
ServiceBinary  = %12%\iaStorAC.sys 
LoadOrderGroup = SCSI miniport 
AddReg = pnpsafe_pci_addreg

[pnpsafe_pci_addreg]
; Use raw values for BusType, not a DEFINE, ChkInf fails on hex alpha chars 
; BusType_ATA == 0x3, BusTypeATA, BusType_RAID == 0x8, BusType_SATA == 0xb
HKR, Parameters\PnpInterface,  5,  %REG_TYPE_DWORD%,  0x00000001 
HKR, Parameters, BusType, %REG_TYPE_DWORD%,  0x0000000b
; Opt into StorPort's I/O latency cap.
HKR, "Parameters",             "IoLatencyCap",              %REG_TYPE_DWORD%,  0x000001F4 

[iaStorAC_EventLog_inst] 
AddReg = iaStorAC_EventLog_addreg 

[iaStorAC_EventLog_addreg] 
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\drivers\iaStorAC.sys"
HKR,,TypesSupported,%REG_TYPE_DWORD%,7 

;*************************************
;* Service: RstMwService
;*************************************
[RstMwService_inst]
DisplayName   = %RstMwService.ServiceName%
Description   = %RstMwService.ServiceDescription%
ServiceType   = %SERVICE_WIN32_OWN_PROCESS%
StartType     = %SERVICE_AUTO_START%
ErrorControl  = %SERVICE_ERROR_NORMAL%
ServiceBinary = %13%\RstMwService.exe

[RstMwService_EventLog_inst] 
AddReg = RstMwService_EventLog_addreg 

[RstMwService_EventLog_addreg] 
HKR,,EventMessageFile,%REG_EXPAND_SZ%,"%%SystemRoot%%\System32\IoLogMsg.dll;%%SystemRoot%%\System32\RstMwEventLogMsg.dll"
HKR,,TypesSupported,%REG_TYPE_DWORD%,0x1F
HKR,,CategoryCount,%REG_TYPE_DWORD%,1

;*************************************
;* Hardware install section
;*************************************
[AHCI_inst.NTamd64.HW]
AddReg = msi_addreg
AddReg = storport_addreg
AddReg = etw_rst_addreg

[msi_addreg]
HKR, Interrupt Management, 0x00000010
HKR, Interrupt Management\MessageSignaledInterruptProperties, 0x00000010
HKR, Interrupt Management\MessageSignaledInterruptProperties, MSISupported, %REG_TYPE_DWORD%,   1
HKR, Interrupt Management\MessageSignaledInterruptProperties, MessageNumberLimit, %REG_TYPE_DWORD%,   80
HKR, Interrupt Management\Affinity Policy, 0x00000010
HKR, Interrupt Management\Affinity Policy, DevicePolicy, %REG_TYPE_DWORD%, 5 ;IrqPolicySpreadMessagesAcrossAllProcessors

[storport_addreg]
; Enables/Disables Idle Power Management for StorPort
HKR, StorPort, EnableIdlePowerManagement, %REG_TYPE_DWORD%, 0x00000001
; Force StorPort to keep all sense data in Pre-Win8 OSes (max value is 255)
HKR, StorPort, TotalSenseDataBytes, %REG_TYPE_DWORD%, 0x000000FF

[etw_rst_addreg]
; Configuring and Starting an AutoLogger Session
; LogFileMode = Buffering Mode | EVENT_TRACE_ADDTO_TRIAGE_DUMP(0x80000000) | EVENT_TRACE_NO_PER_PROCESSOR_BUFFERING (0x10000000)
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST, LogFileMode, %REG_TYPE_DWORD%, 0x90000400
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST, FileName
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST, Guid, %REG_TYPE_SZ%, "{347659f2-c334-46ab-b19e-a451e851c695}"
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST, Start, %REG_TYPE_DWORD%, 0x00000001
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST, BufferSize, %REG_TYPE_DWORD%, 0x00001388
; Configure provider using GUID
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST\{67c35f2c-bae5-4bc8-a999-d339e5ef89ac}, EnableProperty, %REG_TYPE_DWORD%, 0x00000000
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST\{67c35f2c-bae5-4bc8-a999-d339e5ef89ac}, Enabled, %REG_TYPE_DWORD%, 0x00000001
; Level = TRACE_LEVEL_INFORMATION
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST\{67c35f2c-bae5-4bc8-a999-d339e5ef89ac}, EnableLevel, %REG_TYPE_DWORD%, 0x00000004
; Flags = ALL
HKLM, System\CurrentControlSet\Control\WMI\Autologger\IntelRST\{67c35f2c-bae5-4bc8-a999-d339e5ef89ac}, EnableFlags, %REG_TYPE_DWORD%, 0x0000FFFF

;******************************************************************************
;*
;* Strings
;*
;******************************************************************************
[Strings] 
INTEL = "Intel Corporation"
diskId1 = "RST AHCI Installation Disk" 

iaStorAC.ServiceName = "Intel(R) Chipset SATA/PCIe RST Premium Controller"

RstMwService.ServiceName = "Intel(R) Storage Middleware Service"
RstMwService.ServiceDescription = "RPC endpoint service which allows communication between driver and Windows Store Application"
RstMwService.EventLogSourceName = "RST Middleware"

PCI\VEN_8086&DEV_A282&CC_0106.DeviceDesc = "Intel(R) 300 Series Chipset Family SATA AHCI Controller"
PCI\VEN_8086&DEV_34D3&CC_0106.DeviceDesc = "Intel(R) 400 Series Chipset Family SATA AHCI Controller"
PCI\VEN_8086&DEV_02D3&CC_0106.DeviceDesc = "Intel(R) 400 Series Chipset Family SATA AHCI Controller"
PCI\VEN_8086&DEV_06D2&CC_0106.DeviceDesc = "Intel(R) 400 Series Chipset Family SATA AHCI Controller"
PCI\VEN_8086&DEV_06D3&CC_0106.DeviceDesc = "Intel(R) 400 Series Chipset Family SATA AHCI Controller"
PCI\VEN_8086&DEV_A382&CC_0106.DeviceDesc = "Intel(R) 400 Series Chipset Family SATA AHCI Controller"
PCI\VEN_8086&DEV_43D2&CC_0106.DeviceDesc = "Intel(R) 500 Series Chipset Family SATA AHCI Controller"

SPSVCINST_ASSOCSERVICE = 0x00000002 
REG_TYPE_SZ = 0x00000000 
REG_MULTI_SZ = 0x00010000 
REG_EXPAND_SZ = 0x00020000 
REG_TYPE_DWORD = 0x00010001 
SERVICE_KERNEL_DRIVER  = 1 
SERVICE_FILE_SYSTEM_DRIVER = 2
SERVICE_WIN32_OWN_PROCESS = 0x00000010
SERVICE_BOOT_START = 0
SERVICE_AUTO_START = 2
SERVICE_DEMAND_START = 3
SERVICE_ERROR_NORMAL = 1
